Software description

1. Installs
   1. Windows 7
   2. TesterXpWin7\_3.3 (TclTk8.4, RLSerial, RLExPio, RLTime, BTL, RLStatus, RLDxc4, RLEtxGen)
2. AT software package
   1. C:\ AT-ETX5300A-MC-4XFP
3. Operation file
   1. 1-Tester.tcl

The Tester performs tests of Main Cards. The Station Clock Test uses DXC-4/4 based Generator as a source of the clock. The 10GbEthernet tests use 1GbEth Generator, based on ETX204, and an Convertor 1G --> 10G, based on ETX220.